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KENTUCKY POLLUTION DISCHARGE
ELIMINATION SYSTEM (KPDES)

Pre-Mining Survey Map (PMSM) Form
For
In-stream Monitoring Permit Requirements


	In-Stream Monitoring is required as one means of determining compliance with the narrative water quality standard for specific conductance. These requirements will be imposed on all new or expanded active surface mining areas draining to a continuously flowing sediment control structure, new or expanded underground mines, new or expanded coal preparation plants, and all discharges to a designated Outstanding State Resource Water (OSRW) that supports a threatened or endangered species. 
These monitoring requirements include physical, chemical and biological data to be collected for each receiving stream impacted by the permitted activity. The permittee is required to conduct a minimum of a single pre-mining sampling event to establish the baseline conditions to which subsequent annual sampling events are compared to determine compliance. To ensure the data collected is complete, accurate, and representative of the receiving stream, the permittee is required to develop and submit a Pre-Mining Survey PMSM form and map for review and acceptance. 
Physical/chemical samples are to be collected in accordance with the following Standard Operating Procedures (SOPs): (1) Sampling surface waters, (2) In situ Water Quality Measurements and Meter Calibration for Lotic Waters, (3) Sample Control and Management, and (4) Measuring Stream Discharge. Biological sampling shall be performed annually during the appropriate index period; i.e. Headwater – Feb 15th thru May 31st; Wadeable – May 1 thru Sept 30th. Biological samples shall be collected in accordance with: (1) Methods for Conducting Resource Extraction Individual Permit Intensive Surveys in Non-OSRW Streams of the Eastern Kentucky Coalfields; (2) Methods for Conducting Resource Extraction Individual Permit Intensive Surveys in Non-OSRW Streams of the Western Kentucky Coalfields.  All biological activities shall be performed by a qualified biologist. These SOPs may be found at:
 https://eec.ky.gov/Environmental-Protection/Water/PermitCert/KPDES/Pages/Mining.aspx.
To assist the permittee in developing a PMSM and to allow for an expeditious review by DOW, this form has been developed to ensure all necessary information has been included. In addition to this form, the permittee shall attach the following document:
· A PMSM Map illustrating all existing and proposed outfalls associated with the in-stream monitoring, hollow fills, and in-stream monitoring point locations.

	[bookmark: _Hlk233100858]Reason for Submittal (include the reason for the in-stream monitoring requirement and if this request is for new or expanded operations):

	SECTION I – PERMIT INFORMATION
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SECTION IV – IN-STREAM MONITORING LOCATIONS INFORMATION

	ID Number
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	At a minimum, one in-stream monitoring point directly below the outfall along with one downstream monitoring point of the receiving stream located after the confluence but above any tributaries is required. If two locations are not feasible, please explain in the comments field below.

	Comments: 

	SECTION V –PMSM FORM PREPARER INFORMATION

	First Name:      
	Last Name:      
	Company Name:      

	Mailing Address:      
	City:      
	State:      
	Zip Code:      

	Email Address:      
	Business Phone:      

	SECTION VI – CERTIFICATION

	I certify under penalty of law that this document and all attachments were prepared under my direction or supervision in accordance with a system designed to assure that qualified personnel properly gather and evaluate the information submitted. Based on my inquiry of the person or persons who manage the system, or those persons directly responsible for gathering the information submitted, is to the best of my knowledge and belief, true, accurate, and complete.  I am aware that there are significant penalties for submitting false information, including the possibility of fine and imprisonment for knowing violations.
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This completed application form and attachments should be emailed to:  SWPBSupport@ky.gov .  Questions should be directed to the Surface Water Permits Branch at (502) 564-3410.
PMSM FORM 

PMSM FORM	

6/23/2026
6/23/2026
KENTUCKY POLLUTANT DISCHARGE ELIMINATION SYSTEM 
PMSM FORM – INSTRUCTIONS

Reason for Submittal: Please describe the reason the in-stream monitoring is required and if this request is for new or expanded operations.
SECTION I – PERMIT INFORMATION
Agency Interest ID: Provide the AI ID assigned by DOW for this facility, if known.
KPDES Permit ID: Provide the KPDES Permit ID assigned by DOW for this facility, if known.
SMCRA Permit No.: Provide the SMCRA Permit No. assigned by DNR for this facility.
DNR Actions: List all DNR permitting actions, (i.e. amendments, major revisions, minor revisions) associated with this request.
County: Provide the county where the facility is located.
SECTION II – FACITLITY OPERATOR INFORMATION
Provide the Company name, Contact person, and all associated contact information.
SECTION III - GENERAL SITE LOCATION INFORMATION
Facility Address: Provide the facility address and/or the nearest intersection.
Facility Coordinates: Coordinates shall be in decimal degrees, 5 digits after the decimal is required throughout the form.
SECTION IV – IN-STREAM MONITORING LOCATIONS INFORMATION
Complete one line for each in-stream monitoring point location. At a minimum, one in-stream monitoring point directly below the outfall along with one downstream monitoring point in the receiving stream located after the confluence but above any tributaries is required. If two locations are not feasible, please explain in the comment field below. 
ID Number: Provide the identification number which is a 3-digit number starting with I01 (I = In-stream), assigned to the in-stream monitoring point location.
Receiving Water Name: Provide the name of the receiving water being monitored at this location.
Latitude/Longitude: Provide the latitude and longitude (in decimal degrees only) of the monitoring point location.
Outfalls Covered: Provide all outfalls associated with this in-stream monitoring point location.
Headwater or Wadeable Stream: Identify if stream location to be sampled is a Headwater or Wadeable stream segment.
Comments: Provide any necessary comments.
SECTION V – PMSM FORM PREPARER INFORMATION
Provide the name, company name and all associated contact information of the person who prepared the PMSM.
SECTION VI – CERTIFICATION
Provide all requested information.
This completed application form and attachments should be emailed to: SWPBSupport@ky.gov. Questions should be directed to the Surface Water Permits Branch at (502) 564-3410.
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